ERROE CODE E.0C1\n\n During acceleration Overcurent shut-off\n\n -DESCRIPTION-\n When the inverter output current reaches or exceeds approximately 200% of the rated current,the\n protective circuit is activated to stop the inverter output.\n\n -CORRECTIVE ACTIONS-\n Increase acceleration time.
ERROR CODE E.0C2\n\n During constant speed Overcurent shut-off\n\n -DESCRIPTION-\n When the inverter output current reaches or exceeds approximately 200% of the rated current,the\n protective circuit is activated to stop the inverter output.\n\n -CORRECTIVE ACTIONS-\n Keep load stable.
ERROR CODE E.0C3\n\n During deceleration Durng stop Overcurent shut-off\n\n -DESCRIPTION-\n When the inverter output current reaches or exceeds approximately 200% of the rated current,the\n protective circuit is activated to stop the inverter output.\n\n -CORRECTIVE ACTIONS-\n Increase deceleration time.Check brake operation.  
ERROR CODE E.0V1\n\n During acceleration Regenerative overvoltage shut-off\n\n -DESCRIPTION-\n If regenerative energy from the running motor causes the inverter's internal main circuit DC   \n voltage to reach or exceed the specified value is activated to stop the inverter \n output.This may also be activated by a surge voltage generated in the power supply system.\n\n -CORRECTIVE ACTIONS-\n Increase acceleration time. 
ERROR CODE E.0V2\n\n During constant speed Regenerative overvoltage shut-off\n\n -DESCRIPTION-\n If regenerative energy from the running motor causes the inverter's internal main circuit DC   \n voltage to reach or exceed the specified value is activated to stop the inverter \n output.This may also be activated by a surge voltage generated in the power supply system.\n\n -CORRECTIVE ACTIONS-\n Keep load stable. 
ERROR CODE E.0V3\n\n During deceleration Durng stop Regenerative overvoltage shut-off\n\n -DESCRIPTION-\n If regenerative energy from the running motor causes the inverter's internal main circuit DC   \n voltage to reach or exceed the specified value is activated to stop the inverter \n output.This may also be activated by a surge voltage generated in the power supply system.\n\n -CORRECTIVE ACTIONS-\n Increase deceleration time. Reduce braking duty. 
ERROR CODE E.THM\n\n Overload shut-off Motor (electronic overcurrent protection)\n\n -DESCRIPTION-\n The electronic overcurrent protection in the inverter detects motor overheat due to overload or\n cooling capability reduced during constant-sppend operation. When 85% of the     \n preset value is reached, pre-alarm(TH indication)occurs.When the specified value is reached, \n the protective circuit is activated to stop the inverter output.When a special motor such as a \n multi-pole motor or more than one motor is run, the motor cannot be proteceted by the \n electronic overcurrent protection. Provide a thermal relay in the inverter output circuit\n\n -CORRECTIVE ACTIONS-\n Reduce load. Increase motor and inverter capacities.  
ERROR CODE E.FIN\n\n Fin overheat\n\n -DESCRIPTION-\n If the cooling fin overheats, the temperature sensor is activated to stop the inverter out put.\n\n -CORRECTIVE ACTIONS-\n Set ambient temperrature within.
ERROR CODE E. BE\n\n Break transistor alarm detection\n\n -DESCRIPTION-\n If the brake circuit fault has occurred deu to damaged break transistors,ect.,this function    \n stop the inverter output.In this case, the inverter power must be switches off immediately.\n\n -CORRECTIVE ACTIONS-\n Change inverter.
ERROR CODE E. GF\n\n Output side ground fault overcurrent protection\n\n -DESCRIPTION-\n This function stops the innverter output if a ground fault occurring in the inverter output    \n (load)side when starting the inverter. A ground fault occurring at low ground    \n resistance may activate the overcurrent protection(OC1toOC3).\n\n -CORRECTIVE ACTIONS-\n Resolve ground faults.
ERROR CODE E.OHT\n\n External thermal relay operation\n\n -DESCRIPTION-\n If the extermal relay designed for motor overheat protection or the internally mounted         \n temperature relay in thne motor swithes on (relay contacts "open"),the inverter  \n output can be stoped if those contacts had been entered into the inverter. If the relay      \n contacts are reset automatically, the inverter will not restart unless it is reset.\n\n -CORRECTIVE ACTIONS-\n Reduce load and frequency of poeration.
ERROR CODE E.OLT\n\n During acceleration Stall prevention opretion\n\n -DESCRIPTION-\n If a current more than 150% of the rated inverter current flows in the motor, this function    \n lowers the frequency until the load current reduces to prevent the inverter from \n resulting in overcurrent shut-off.When the load current has reduced below 150%, this function\n increases the frequency again to accelerate and poerate the inverter up to the set frequency.\n\n -CORRECTIVE ACTIONS-\n Reduce load. Increase motor and inverter capacities.
ERROR CODE E.OLT\n\n During constant-speed operation Stall prevention opretion\n\n -DESCRIPTION-\n If a current more than 150% of the rated inverter current flows in the motor, this function    \n lowers the frequency until the load current reduces to prevent overcurrent       \n shut-off. When the oad current has reduced below 150%, this function increases the frequency \n up to the set value. \n\n -CORRECTIVE ACTIONS-\n Reduce load. Increase motor and inverter capacities.
ERROR CODE E.OLT\n\n During deceleration Stall prevention opretion\n\n -DESCRIPTION-\n If the regenerative energy of the motor has increased above the break capability, this function\n increases the frequency to prevent overvoltage shut-off. If a current more than  \n 150% of the rated inverter current flows in the motor, this function increase the frequency  \n until the load curent reduces to prevent the inverter resulting in overcurrent shut-off.       \n When the load current has reduced below 150%, this function dereases the frequency again.\n\n -CORRECTIVE ACTIONS-\n Reduce load. Increase motor and inverter capacities.
ERROR CODE E. LF\n\n Open output phase protection\n\n -DESCRIPTION-\n This function stops the inverter output when any of the three phases(U,V,W)on the inverter's   \n output side (load side) opens.\n\n -CORRECTIVE ACTIONS-\n Repair open phase.





